|  |  |
| --- | --- |
| **Specifications** | |
| Panel Size: | (1U) 19" x 1.75" x 1.5" |
| Panel color/material: | black/metal |
| Fans: | 6 - SL40B Blue LED fans |
| Fan Speed: | 4000 RPM |
| Air Flow: | 31.2 CFM |
| Noise: | 20 dBA |
| Power Supply: | 100-240 VAC - 12 VDC |
| Power Supply Plug Type: | NEMA 1-15P |
| Current draw: | 1.5A |
| Power consumption: | 4.5w |
| Grills/Guards: | Black Wire |

Rack Mount Set RM-20/ RM-40

HEIGHT:

4 HU

RM-20: TubeMeister 18, TubeMeister Deluxe 20

RM-40: TubeMeister 36, GrandMeister 36, TubeMeister Deluxe 40, GrandMeister Deluxe 40

COOLING:

Only use in combination with rack fans! We suggest to install a rack fan above the amp.

WEIGHT:

RM-20 (Set): 700 gr. / 1,54 lbs.

RM-40 (Set): 500 gr. / 1,10 lbs.

NOTE: Amp, rack and rack fan are not included.