



\* Model No.

**SL480B – Blue fans**

**SL480G – Green fans**

**SL480P – Purple fans**

**SL480R – Red fans**

|  |  |
| --- | --- |
| Panel SIze:  | (2U) 19" x 3.5" x 1.5" |
| Panel Color/Material:  | Black/Lexan |
| Fans:  | 4 |
| Fan Color | Blue, Green, Purple, Red |
| Fan Size:  | 80mm x 80mm x 25mm  |
| Fan Speed:  | 1800 RPM |
| Air Flow: | 86.8 CFM  |
| Noise: | 26 dBA  |
| Bearings:  | Hydraulic |
| Thermal Probe length | n/a |
| Power Supply:  | 100-240 VAC/12VDC/5VDC  |
| Power Supply Cable length | AC-60" DC-36"  |
| Current draw: | .64A |
| Power consumption:  | 7.68w |
| Grills/Guards: | Black Wire  |